Scans for Fe and [1b10] Y were done with LR=50, all others with LR=150.  This should not lead to any important differences as the calculations are converged to the required accuracy (0.01T) at LR=50.
