CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2/conf/instr/spect/uxnmr.info
Date         : Tue Jan 28 14:51:04 2014
Release      : TOPSPIN Version 3.2-pl2
Installed in : /opt/topspin3.2
Host         : nmrpc
OS           : CentOS release 5.9 (Final)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Administrator)
Description  : AVANCE III HD
Location     : Imperial College London
System       : Avance III NMR spectrometer
1H-frequency : 500.13 MHz
Order Number : 10101142 GH000513
Configured in: /opt/topspin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.253
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/03358 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.2 REC-1  AQS RXAD/2 600 Z130588/551 ECL 00.02
     3   0x34 0xd6   0x1        X  2.0 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/00760 ECL 02.02 FPGA-Vs=20121030
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0971 W1345096/0971 ECL 30:
- TCP/IP address = 149.236.99.254
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0971 ECL 30
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1725 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7084 ECL 50
- QNP-Accessory  : 1 X-input and 1 H-input
LTRX Z109889/00483 ECL 03.01:
- TCP/IP address = 149.236.99.21
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00483 ECL 03.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.21
- ELCB firmware version = 20130320
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00483 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/01406 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/01618 ECL 01.04

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.21

Bruker Automatic Changer: device connected to 149.236.99.253:/dev/tty04
- Capacity: 60 holders
- Firmware: 20040805
- use BACS air  = yes
- BACS sx delay = 1 s
- Sample Rail fast changer mode = no

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.1%/-0.1deg, reflection meter)
                 PN=Z103204, SN=00266 from 20130514
    Module  2 : 2H
                 PN=Z003472, SN=01159 from 20130412
    Module  3 : XBB19F 2HS
                 PN=Z003505, SN=01284 from 20130415


Frequency generation:
- F1: for SGU
- F2: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254)
SGU1 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254) amplifier X-300W uses blanking 1
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254) amplifier 2H-150W uses blanking 4
transmitter 2 (BSMS/2 LOCK TRANSCEIVER 500 Z109889/00483 at TCP/IP 149.236.99.21) amplifier 2H-5W needs no blanking

Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254 amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254 amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
BLAXH2H300/100/150 E 200-600MHZ W1345096/0971 at TCP/IP 149.236.99.254 amplifier 2H-150W at blanking 4 can be routed to switchbox output 5 (unknown)

