Figure 7

Figure 7(c) has two datasets. One is simulated microwave field intensity. One is change in absorption.

Change in absorption data:

this data is the same as is used in figure 1, the data and the processing code are in this folder.


microwave field simulations:

The simulations were performed using HFSS Ansys. The extracted field strength vs micowave frequency for the two antennas A1 and A2 are in files "HFSS_A1.csv" and "HFSS_A2.csv"

The files are organised as 

Phase [deg]	Freq [GHz]	av_E_sample_mag_x []	av_E_sample_mag_y []	av_E_sample_mag_z []


for each frequency point the field intensity (E_x^2+E_y^2+E_z^2) was found, and is plotted in figure 7(c). 