The xlsx file shows the results of the simulation for the estimation of the ultra-low-grade heat recovery and storage using aqueous solution of (i) CaCl2, (ii) LiCl, (iii) HCO2K when using single and double regenerators and energy is transport between heat supply and end-user every 1, 2, 3, 4 and 5 days