Supporting data for “Shear banding as a cause of nonmonotonic stress relaxation after flow cessation”

Basic code in this parent directory
Usage:
runs.sh parameters.dat

To reproduce specific figures, please see subfolders for data, simulation code and example simulations
