The folder (and sub folders) contains all of the raw data used to extract the sideband amplitudes.

Each subfolder is named by the wavelgnth of the excitations laser (note, we used a frequency doubled laser, but record the fundamental wavelength. That means these numbers need to be divided by 2 to get the wavelenght of the light hitting the sample).

Inside each subfolder is a series of files. Each of these files corresponds to a different temperature (frequency) of the etalon.
The tempearture used is saved in the file.
The conversion from frequency to temperature is in the analysis code.

Each file contains the counts with and without the microwave field at a given etalon temperature. The applied microwave power is varied within each file.
Note the microwave power quoted refers to the power before the amplifier, and needs to be increased by 24 dB to get the power going into the sample.

the file
"sideband rollover analysis v3.nb"
contains the code used to analyse all of the data in these folders and fit the spectra. These fitted values are what is extracted and put in the parent folder to this sub folder.
This file also contians the code to make the plot in figure 1.

